# About this Release

This In-Sight 25.3.0 release adds the following bug fixes and improvements:

New features in the In-Sight Vision Suite:

- Added the Enterprise Connectivity utility for managing MQTT Message Queue Telemetry Transport (MQTT) is a lightweight messaging protocol used to send and receive data between devices. connections.

- Added the Services & Ports utility for selective port and service management.

- Added an Export User Files option in the Backup utility, allowing you to access user files from backups without a connected vision system.

- You can define the location for the Backup and Restore files.

- The Time Settings utility now includes an option to disable DST compensation for the time zone.

- The Calibration Grid utility is available for the emulator.

- Improved Local Device file path handling on the emulator.

- Audit log now includes cell name changes.

- Added option to set up FTP and SFTP server from In-Sight Vision Suite.

- Added Omnidirectional scanning option to the ReadIDMax function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. in Spreadsheet and the ReadID tool in EasyBuilder.

- Added audit logging to metric A metric is a data value with additional context such as type or properties that explain what the value means and how it is used or shown, helping systems understand and work with the data correctly. API.

- Changes to ApplyAcquisitionSettings take effect quicker for In-Sight 8900 series vision systems.

- Improved file path handling on emulators.

- The X and Y ROI values for tools can exceed 9999 to accommodate new, higher resolution cameras.

New features and improvements in In-Sight Spreadsheet:

- Added Profile Job A job is a user-configured program in In-Sight 3D EasyBuilder consisting of functions and designed for specific applications. You can create and edit jobs using the In-Sight 3D EasyBuilder interface, and load them on a vision system for deployment in a live environment. tool to Spreadsheet under the View menu.

- Added single character training to the ViDiELRead tool.

- Added dot grid option to the CalibrateGrid function.

- The CalibrateGrid function allows you to define grid axes.

- Added result chunking for the WriteResultsBuffer function for all protocols.

- Added drag-and-drop job loading.

- Blob A blob is a group of pixels on the image that form a distinct pattern, typically used to represent objects, features, or areas of interest in object detection and segmentation tasks. functions can now utilize the full ROI.

- Added Timer function.

- The element size of the CombineOutputBuffers and FormatInputBuffer functions is increased.

- The ExtractDistanceHistogram3D function now returns a chart layer instead of a SVG format.

- The output delay with WriteDiscrete function is now calculated from the trigger for L38 and Line Scan vision systems and is now consistent with area scan In-Sight vision systems.

- Added Compare Jobs function that allows you to compare two jobs.

- You can now load jobs by dragging and dropping them into Spreadsheet.

New features and improvements in In-Sight EasyBuilder:

- The Job Validation application step was added to allow users to perform job validation.