# Number of Rows (Line Scan)

Defines the number of lines to acquire to create the full line scan image.

The available values are 8–16376, but not all values are valid. The spreadsheet user interface marks invalid values with a red exclamation point.

Determining Valid Values

To determine valid values, do the following calculation:

1. Choose a value.

2. Add 4 to your chosen value.

3. Divide the sum by 12.

   If the result is an integer, the setting is valid.

The smallest practical value is 8, so 8, 20, 32, ..., 16376 are valid values.

Note: If you choose a smaller frame length option in the Camera Configuration utility, the maximum number of rows decreases accordingly.