# Result Queue

The Result Queue creates a filmstrip on the WebHMI The operator interface through which the operator interacts with the vision system. about the results.

Results Queue Settings:

Number | Element | Description
1 | Enable result queue | Enables/disables the result queue in the WebHMI. The default setting is disabled.
2 | Mode | Sets what kind of results show up on the result queue. You can choose from the following: Pass and Fail Results Fail Results Pass Results Separate Pass and Fail Results The default setting is Pass and Fail Results.
3 | Queue Size | Sets the queue size, which means how many results you can see in the result queue. The default value is 10 results.
4 | Pass Size | Sets the queue size, which means how many pass results you can see in the result queue. The default value is 1 results.
5 | Fail Size | Sets the queue size, which means how many fail results you can see in the result queue. The default value is 9 results.
6 | Queue offline results | Enables/disables to queue the offline results.
7 | Keep first results | Enables/disables keeping the first results in the result queue.
8 | Clear when placed in online mode | Clears the result queue when you set the vision system to online mode.
9 | Result Condition | Conditions the result queue. Click Select Cell to watch that cell. You can condition the cell watching with the following options: Fail cell with #ERR Fail cell with value < 0 Fail cell with value = 0 Fail cell with value > 0

To add a Result Queue:

1. Navigate to Sensor menu and select Result Queue Settings.

2. Enable the Enable result queue checkbox.

   Note: You must enable the Result Queue for the Pass function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. to work.

3. Adjust your settings and click OK.