The following table describes the High Dynamic Range (HDR) settings available on the Acquisition Acquisition is the process or result of the vision system acquiring a new image. panel:

Setting | Description
--- | ---
HDR Mode | Enables or disables High Dynamic Range (HDR) processing. The following options are available: None HDR HDR+ Note: HDR+ is only available on IS3800 models. HDR is not available on color units. If you load a job A job is a user-configured program in In-Sight Spreadsheet consisting of functions and designed for specific applications. You can create and edit jobs using the In-Sight Spreadsheet interface, and load them on a vision system for deployment in a live environment. with HDR+ settings on a vision system that only supports HDR, the job settings automatically switch to HDR. If you load a job with HDR or HDR+ settings on a vision system that does not support any HDR, the job settings automatically switch to None. If you load a job with HDR+ settings with an incompatible kernel A kernel is a rectangular array of numbers that defines the processing neighborhood for operations performed on each pixel location in an image. size setting on a supported vision system, the kernel size is automatically set to default.