# Get Online

Returns the Online state of the vision system. For more information, see Online and Offline States.

## Get Online Inputs

Syntax: GO

## Get Online Outputs

Returns the Online state of the vision system.

Online State | Description
--- | ---
0 | The vision system is currently Offline.
1 | The vision system is currently Online.

## Get Online Example

To determine the Online state of the vision system, issue the following command: GO

The vision system responds with 1, indicating that the vision system is currently Online.