# LineFromNPoints

Constructs a line from a list of points.

Inputs

The LineFromNPoints function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. has the following syntax:

LineFromNPoints(Image, Point X 0, Point Y 0, Point X 1, Point X 1, Point Y 1, Point X 2, Point Y 2, [Point X 3, Point Y 3, …, Show])

See the table for a description of the available parameters.

Parameter | Description
Image | This argument must reference a spreadsheet cell that contains a valid Image data structure. By default, the cell referenced is cell A0, containing the AcquireImage function.
Point 0 | Specifies the coordinates of the first point.
Point X 0 | The X coordinate of the first point.
Point Y 0 | The Y coordinate of the first point.
Point 1 | Specifies the coordinates of the second point.
Point X 1 | The X coordinate of the second point.
Point Y 1 | The Y coordinate of the second point.
Point 2..N | Specifies the coordinates of any additional points.
Point X N | The X coordinate of the Nth point.
Point Y N | The Y coordinate of the Nth point.
Show | Specifies the graphics items to be displayed on a permanent basis.
0 = hide all | All graphics items are hidden except when the cell containing the LineFromNPoints function is the active cell in the spreadsheet.
1 = result graphics only | The fitted line graphic is displayed at all times. The input points are only displayed when the cell containing the LineFromNPoints function is the active cell in the spreadsheet.
2 = input and result graphics | The fitted line and the input points are displayed at all times.

Outputs

Returns | A LineFit data structure if two or more valid points are included in data, or #ERR if only one or no valid point is included in data.
Results | When the function is initially inserted into a cell, the following LineFit Vision Data Access functions are automatically inserted into the spreadsheet to create a result table:
Label | Function | Description
X0 | GetX(LineFit, 0) | The X coordinate of the first endpoint.
Y0 | GetY(LineFit, 0) | The Y coordinate of the first endpoint.
X1 | GetX(LineFit, 1) | The X coordinate of the second endpoint.
Y1 | GetY(LineFit, 1) | The Y coordinate of the second endpoint.
Chi2 | GetChi2(LineFit) | The sum of the squares of the distances from the points to the line.
Additional data elements can be accessed using the following Vision Data Access functions:
Label | Function | Description
--- | --- | ---
Distance | GetDistance(LineFit, Index) | The distance between the indexed point and the line.
MaxDist | GetMaxDist(LineFit) | The point that is farthest from the line.
MaxDistIndex | GetMaxDistIndex(LineFit) | The index of the point that is farthest from the line.
NPointsUsed | GetNPointsUsed(LineFit) | The number of points used to compute the line.