# TransInspEdgeWidthToWorld

Applies a coordinate transform to an InspectEdgeWidth data structure.

Note: The output of any vision tool that reports in real-world coordinates cannot be used as a fixture A fixture is a coordinate location on the image that keeps the tool in the place determined by the fixture. or region input to another vision tool.
Inputs

The TransInspEdgeWidthToWorld function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. has the following syntax:

TransInspEdgeWidthToWorld(Calib, InspectEdgeWidth)

See the table for a description of the available parameters.

Parameter | Description
Calib | A reference to a spreadsheet cell containing a valid Calib data structure.
InspectEdgeWidth | A reference to a spreadsheet cell containing a valid InspectEdgeWidth data structure.

Outputs

Returns | InspectEdgeWidth structure translated to real-world coordinates, or #ERR if any of the input parameters are invalid.