# ApplyAcquisitionSettings3d

The ApplyAcquisitionSettings3d function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. allows you to modify the acquisition Acquisition is the process or result of the vision system acquiring a new image. settings of the vision system. The function supports a subset of the settings in the Acquisition panel.

When you change the settings using this function, the vision system immediately stops the ongoing acquisition to apply the new settings. When the vision system finishes the reconfiguration, it automatically resumes the acquisition. During the short time when the ongoing acquisition stops, the vision system discards all triggers and these triggers are not considered missed triggers. For this reason, Cognex recommends you to stop the production line when performing changes.

If you have more than one ApplyAcquisitionSettings3d functions in the spreadsheet, the vision system uses only the last updated value. For this reason, Cognex recommends to have only one ApplyAcquisitionSettings3d function enabled at a time.

The values of the field correction settings are temporary, and they do not affect the field correction values stored on the vision system. When you restart the vision system or change jobs, the original field correction value is restored. Additionally, when exporting the field correction to a file, the original field correction value is used instead of the value configured by the ApplyAcquisitionSettings3d function.