View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do Multiple Read Setups interact with the Timeout setting?

When Multiple read setups are enabled, the timeout affects each setup individually, and not all the setups as a whole. The result is that the total time spent on reading in one trigger cycle is the product of the number of enabled setups and the timeout.

Note: DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503