# Inspection Results

Inspection Results
Offset (bytes) | Field | Data Type
--- | --- | ---
0x00 | Payload Version 1 | uint8
0x01 | Application | uint8
0x02 | Program | uint8
0x03 | Inspection Status Code | uint8
0x04 | Identified Class Enumeration | uint8
0x05 | Identified Class Confidence | uint8
0x06 | Class Name (ASCII) | String
0x93

Application - 1 byte
1 | Anomaly Detector
2 | 2-Class Classifier

Inspection Status Code - 1 byte
0 | Inspection Valid
1 | Sensor Untrained
2 | Fixture Not Found
3 | ROI Outside Image
4...255 | Reserved

Identified Class Enumeration - 1 byte
Anomaly Detector | 2-Class Classifier
0 | Reserved | 0 | Unclassified
1 | OK | 1 | OK
2 | NG | 2 | NG
4...254 | Reserved | 4...254 | Reserved
255 | Error | 255 | Error