# TCP/IP Inputs

The TCP/IP commands are a series of ASCII characters terminated by a single newline. Unrecognized commands or additional terminators are discarded and ignored. The SET_PROGRAM[#] command changes to the program slot indicated by the #. The # is an integer value and can be zero-padded or not. This means that both the SET_PROGRAM[01] and SET_PROGRAM[1] are allowed.

The text name for the trigger command is configurable. Characters are limited to the printable ASCII characters. Unicode text is not allowed.