# Add Hybrid Switch

If the switch list does not contain switches or contains misconfigured switches, you can discover and configure switches.

To add a hybrid switch:

1. Click Discover Devices.

2. Find the switch whose state is Misconfigured in the switch list and click the Edit Switch Network Settings icon next to it.

   The Edit Switch Network Settings window pops up.

3. Disable the Use DHCP toggle.

4. Edit the IP Address, Subnet Mask, and Gateway so that the switch is on the correct local or remote subnet.

5. Click Submit.

   The state of the switch in the switch list is now In Local Subnet.