# Inspect Textures — Steps

Note: For more information on the specific steps of setting up the tool, see the Using the Red Analyze Tool topics.

1. Add the images for the Textures tutorial.
2. Use the default ROI size, and segment the images by clicking the Scissors icon.
3. Label all of the images as Good.
4. Use the Display Filters to sort the images that contain the word "bad" in their file-name (type 'bad' into the Display field). Label those images as Bad.
5. Train the tool and review the results.
6. Note that the performance is very poor, with the tool reporting nearly all the images as intermediary.
7. Switch the tool to Supervised Mode.
8. In 20 of the "bad" images, label the defective areas with Regions.
9. Train the tool and review the results.
10. If necessary, label additional defective areas and retrain.