# Edge Angle Tolerance

The LineMax tool uses an edge angle tolerance to limit the difference between the gradient vector direction for an edge point and the expected orientation of the line segment. Candidate gradient vectors with a direction within that range are included as inliers to the found line segment.

As you increase the edge angle tolerance, you allow the tool to consider more edge points as inliers and change the location of the found line, as illustrated in the following figure: