# Elasticity

Unless you expect pattern variations that cannot be described using a linear transformation, you should specify a value of 0.0 for elasticity.

If you experience alignment failures or unstable score results, you can begin experimenting with low elasticity values. In general, you should specify the lowest elasticity value that provides stable and consistent alignment results.

If you are expecting significant nonlinear pattern deformation, you should use the PatFlex algorithm.